GROUP = L1_METADATA_FILE
  GROUP = METADATA_FILE_INFO
    ORIGIN = "Image courtesy of the U.S. Geological Survey"
    REQUEST_ID = "0101411199244_00406"
    LANDSAT_SCENE_ID = "LE70330332006290EDC00"
    FILE_DATE = 2014-11-21T22:28:58Z
    STATION_ID = "EDC"
    PROCESSING_SOFTWARE_VERSION = "LPGS_12.5.0"
    DATA_CATEGORY = "NOMINAL"
  END_GROUP = METADATA_FILE_INFO
  GROUP = PRODUCT_METADATA
    DATA_TYPE = "L1G"
    OUTPUT_FORMAT = "GEOTIFF"
    EPHEMERIS_TYPE = "DEFINITIVE"
    SPACECRAFT_ID = "LANDSAT_7"
    SENSOR_ID = "ETM"
    SENSOR_MODE = "SAM"
    WRS_PATH = 033
    WRS_ROW = 033
    DATE_ACQUIRED = 2006-10-17
    SCENE_CENTER_TIME = 17:27:12.9801163Z
    CORNER_UL_LAT_PRODUCT = 39.88081
    CORNER_UL_LON_PRODUCT = -106.09345
    CORNER_UR_LAT_PRODUCT = 39.87372
    CORNER_UR_LON_PRODUCT = -103.31499
    CORNER_LL_LAT_PRODUCT = 37.92115
    CORNER_LL_LON_PRODUCT = -106.06380
    CORNER_LR_LAT_PRODUCT = 37.91454
    CORNER_LR_LON_PRODUCT = -103.36068
    CORNER_UL_PROJECTION_X_PRODUCT = 406500.000
    CORNER_UL_PROJECTION_Y_PRODUCT = 4415100.000
    CORNER_UR_PROJECTION_X_PRODUCT = 644100.000
    CORNER_UR_PROJECTION_Y_PRODUCT = 4415100.000
    CORNER_LL_PROJECTION_X_PRODUCT = 406500.000
    CORNER_LL_PROJECTION_Y_PRODUCT = 4197600.000
    CORNER_LR_PROJECTION_X_PRODUCT = 644100.000
    CORNER_LR_PROJECTION_Y_PRODUCT = 4197600.000
    PANCHROMATIC_LINES = 14501
    PANCHROMATIC_SAMPLES = 15841
    REFLECTIVE_LINES = 7251
    REFLECTIVE_SAMPLES = 7921
    THERMAL_LINES = 7251
    THERMAL_SAMPLES = 7921
    FILE_NAME_BAND_1 = "LE70330332006290EDC00_B1.TIF"
    FILE_NAME_BAND_2 = "LE70330332006290EDC00_B2.TIF"
    FILE_NAME_BAND_3 = "LE70330332006290EDC00_B3.TIF"
    FILE_NAME_BAND_4 = "LE70330332006290EDC00_B4.TIF"
    FILE_NAME_BAND_5 = "LE70330332006290EDC00_B5.TIF"
    FILE_NAME_BAND_6_VCID_1 = "LE70330332006290EDC00_B6_VCID_1.TIF"
    FILE_NAME_BAND_6_VCID_2 = "LE70330332006290EDC00_B6_VCID_2.TIF"
    FILE_NAME_BAND_7 = "LE70330332006290EDC00_B7.TIF"
    FILE_NAME_BAND_8 = "LE70330332006290EDC00_B8.TIF"
    METADATA_FILE_NAME = "LE70330332006290EDC00_MTL.txt"
    CPF_NAME = "L7CPF20061001_20061231.08"
  END_GROUP = PRODUCT_METADATA
  GROUP = IMAGE_ATTRIBUTES
    CLOUD_COVER = 75.00
    IMAGE_QUALITY = 9
    SUN_AZIMUTH = 155.35991405
    SUN_ELEVATION = 38.44085606
  END_GROUP = IMAGE_ATTRIBUTES
  GROUP = MIN_MAX_RADIANCE
    RADIANCE_MAXIMUM_BAND_1 = 293.700
    RADIANCE_MINIMUM_BAND_1 = -6.200
    RADIANCE_MAXIMUM_BAND_2 = 300.900
    RADIANCE_MINIMUM_BAND_2 = -6.400
    RADIANCE_MAXIMUM_BAND_3 = 234.400
    RADIANCE_MINIMUM_BAND_3 = -5.000
    RADIANCE_MAXIMUM_BAND_4 = 241.100
    RADIANCE_MINIMUM_BAND_4 = -5.100
    RADIANCE_MAXIMUM_BAND_5 = 47.570
    RADIANCE_MINIMUM_BAND_5 = -1.000
    RADIANCE_MAXIMUM_BAND_6_VCID_1 = 17.040
    RADIANCE_MINIMUM_BAND_6_VCID_1 = 0.000
    RADIANCE_MAXIMUM_BAND_6_VCID_2 = 12.650
    RADIANCE_MINIMUM_BAND_6_VCID_2 = 3.200
    RADIANCE_MAXIMUM_BAND_7 = 16.540
    RADIANCE_MINIMUM_BAND_7 = -0.350
    RADIANCE_MAXIMUM_BAND_8 = 243.100
    RADIANCE_MINIMUM_BAND_8 = -4.700
  END_GROUP = MIN_MAX_RADIANCE
  GROUP = MIN_MAX_PIXEL_VALUE
    QUANTIZE_CAL_MAX_BAND_1 = 255
    QUANTIZE_CAL_MIN_BAND_1 = 1
    QUANTIZE_CAL_MAX_BAND_2 = 255
    QUANTIZE_CAL_MIN_BAND_2 = 1
    QUANTIZE_CAL_MAX_BAND_3 = 255
    QUANTIZE_CAL_MIN_BAND_3 = 1
    QUANTIZE_CAL_MAX_BAND_4 = 255
    QUANTIZE_CAL_MIN_BAND_4 = 1
    QUANTIZE_CAL_MAX_BAND_5 = 255
    QUANTIZE_CAL_MIN_BAND_5 = 1
    QUANTIZE_CAL_MAX_BAND_6_VCID_1 = 255
    QUANTIZE_CAL_MIN_BAND_6_VCID_1 = 1
    QUANTIZE_CAL_MAX_BAND_6_VCID_2 = 255
    QUANTIZE_CAL_MIN_BAND_6_VCID_2 = 1
    QUANTIZE_CAL_MAX_BAND_7 = 255
    QUANTIZE_CAL_MIN_BAND_7 = 1
    QUANTIZE_CAL_MAX_BAND_8 = 255
    QUANTIZE_CAL_MIN_BAND_8 = 1
  END_GROUP = MIN_MAX_PIXEL_VALUE
  GROUP = PRODUCT_PARAMETERS
    CORRECTION_GAIN_BAND_1 = "CPF"
    CORRECTION_GAIN_BAND_2 = "CPF"
    CORRECTION_GAIN_BAND_3 = "CPF"
    CORRECTION_GAIN_BAND_4 = "CPF"
    CORRECTION_GAIN_BAND_5 = "CPF"
    CORRECTION_GAIN_BAND_6_VCID_1 = "CPF"
    CORRECTION_GAIN_BAND_6_VCID_2 = "CPF"
    CORRECTION_GAIN_BAND_7 = "CPF"
    CORRECTION_GAIN_BAND_8 = "CPF"
    CORRECTION_BIAS_BAND_1 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_2 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_3 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_4 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_5 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_6_VCID_1 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_6_VCID_2 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_7 = "INTERNAL_CALIBRATION"
    CORRECTION_BIAS_BAND_8 = "INTERNAL_CALIBRATION"
    GAIN_BAND_1 = "L"
    GAIN_BAND_2 = "L"
    GAIN_BAND_3 = "L"
    GAIN_BAND_4 = "L"
    GAIN_BAND_5 = "L"
    GAIN_BAND_6_VCID_1 = "L"
    GAIN_BAND_6_VCID_2 = "H"
    GAIN_BAND_7 = "L"
    GAIN_BAND_8 = "L"
    GAIN_CHANGE_BAND_1 = "LL"
    GAIN_CHANGE_BAND_2 = "LL"
    GAIN_CHANGE_BAND_3 = "LL"
    GAIN_CHANGE_BAND_4 = "LL"
    GAIN_CHANGE_BAND_5 = "LL"
    GAIN_CHANGE_BAND_6_VCID_1 = "LL"
    GAIN_CHANGE_BAND_6_VCID_2 = "HH"
    GAIN_CHANGE_BAND_7 = "LL"
    GAIN_CHANGE_BAND_8 = "LL"
    GAIN_CHANGE_SCAN_BAND_1 = 0
    GAIN_CHANGE_SCAN_BAND_2 = 0
    GAIN_CHANGE_SCAN_BAND_3 = 0
    GAIN_CHANGE_SCAN_BAND_4 = 0
    GAIN_CHANGE_SCAN_BAND_5 = 0
    GAIN_CHANGE_SCAN_BAND_6_VCID_1 = 0
    GAIN_CHANGE_SCAN_BAND_6_VCID_2 = 0
    GAIN_CHANGE_SCAN_BAND_7 = 0
    GAIN_CHANGE_SCAN_BAND_8 = 0
  END_GROUP = PRODUCT_PARAMETERS
  GROUP = RADIOMETRIC_RESCALING
    RADIANCE_MULT_BAND_1 = 1.181
    RADIANCE_MULT_BAND_2 = 1.210
    RADIANCE_MULT_BAND_3 = 0.943
    RADIANCE_MULT_BAND_4 = 0.969
    RADIANCE_MULT_BAND_5 = 0.191
    RADIANCE_MULT_BAND_6_VCID_1 = 0.067
    RADIANCE_MULT_BAND_6_VCID_2 = 0.037
    RADIANCE_MULT_BAND_7 = 0.066
    RADIANCE_MULT_BAND_8 = 0.976
    RADIANCE_ADD_BAND_1 = -7.38071
    RADIANCE_ADD_BAND_2 = -7.60984
    RADIANCE_ADD_BAND_3 = -5.94252
    RADIANCE_ADD_BAND_4 = -6.06929
    RADIANCE_ADD_BAND_5 = -1.19122
    RADIANCE_ADD_BAND_6_VCID_1 = -0.06709
    RADIANCE_ADD_BAND_6_VCID_2 = 3.16280
    RADIANCE_ADD_BAND_7 = -0.41650
    RADIANCE_ADD_BAND_8 = -5.67559
  END_GROUP = RADIOMETRIC_RESCALING
  GROUP = PROJECTION_PARAMETERS
    MAP_PROJECTION = "UTM"
    DATUM = "WGS84"
    ELLIPSOID = "WGS84"
    UTM_ZONE = 13
    GRID_CELL_SIZE_PANCHROMATIC = 15.00
    GRID_CELL_SIZE_REFLECTIVE = 30.00
    GRID_CELL_SIZE_THERMAL = 30.00
    ORIENTATION = "NORTH_UP"
    RESAMPLING_OPTION = "CUBIC_CONVOLUTION"
    SCAN_GAP_INTERPOLATION = 2.0
  END_GROUP = PROJECTION_PARAMETERS
END_GROUP = L1_METADATA_FILE
END
